S4C-DP software release notes

Software version:		V1.6
File format:			Zip

Software changes:
Jul 11,2025 V1.6 (Author: Lyman)
   -Add the DP20 product picture in the software
   -Show special item number for the new products DP20 and Atlas

Jun 23,2025 V1.5 (Author: Lyman)
   -Supports DP20
   -Update the dew point calibration interface and the reference dew point input interface.
   -For S230,S231,S220,S211,S215, enable one-point calibration on selected various units：°C Td, °F Td, % rH, mg/m³, g/kg, g/m³, ppm(v) 
   Note: 
   S220_S215_S211：Firmware version V2.2 or above is required.
   S230/S231：Firmware version V2.7 or above is required.

Mar 22,2023 V1.4 (Author: Lyman)
  - Disable the static pressure editing for the sensor integrated pressure sensor in it.
  - Add analog output routing setting
  - Shows QCM low boundary and analog output routing setting on the sensor information dialog

Mar 23,2022 V1.3 (Author: Lyman)
  - Add network check to avoid failure to open the software when there is no network

Mar 31,2022 V1.2 (Author: Lyman)
  - Use Unicode encoding to regenerate the software to avoid random code of special characters in use in other countries
  - When saving sensor information to PDF file, a prompt will be given when the PDF information file of the corresponding sensor already exists
  - When the recording time expires, the logging flag is not reset to "stop"

Nov 01,2021 V1.1 (Author: Lyman)
  - Changed the software name as S4C-DP on main dialog box
  - Changed dew point unit from “Ctd” to “℃ Td” (Ftd to °F Td)and temperature unit from “C” to “℃” (F to °F)
  - Changed the name of com port button on main dialog from “Properties” to “COM Port”
  - Support new sensor S217-IOLINK
  - Removed product pictures from software package and used a new way to show it
  - Add a picture indicator about connecting server when start software